From f527cb6f3345f7faa8e61dd9f3c437437327428c Mon Sep 17 00:00:00 2001
From: Florian Fainelli <f.fainelli@gmail.com>
Date: Mon, 9 Nov 2020 11:41:01 -0800
Subject: [PATCH] ARM: dts: BCM5301X: Update Ethernet switch node name

Update the switch unit name from srab to ethernet-switch, allowing us to
fix warnings such as:

  CHECK   arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dt.yaml
arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dt.yaml:
srab@18007000: $nodename:0: 'srab@18007000' does not match
'^(ethernet-)?switch(@.*)?$'
        From schema:
Documentation/devicetree/bindings/net/dsa/b53.yaml

Reviewed-by: Vladimir Oltean <olteanv@gmail.com>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm5301x.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/bcm5301x.dtsi
+++ b/arch/arm/boot/dts/bcm5301x.dtsi
@@ -485,7 +485,7 @@
 		};
 	};
 
-	srab: srab@18007000 {
+	srab: ethernet-switch@18007000 {
 		compatible = "brcm,bcm5301x-srab";
 		reg = <0x18007000 0x1000>;
 
