From def280c4792262a368c8861312dc6b376181021f Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Mon, 1 Jan 2018 23:10:56 +0100
Subject: sunxi: deactivate binman

Use the old way to generate the images instead of binman.
binman needs python with swig to avoid this host tool dependency use the
old way of generating images.
---
 Makefile | 7 ++++---
 1 file changed, 4 insertions(+), 3 deletions(-)

--- a/Makefile
+++ b/Makefile
@@ -1555,8 +1555,10 @@ endif
 
 ifneq ($(CONFIG_ARCH_SUNXI),)
 ifeq ($(CONFIG_ARM64),)
-u-boot-sunxi-with-spl.bin: spl/sunxi-spl.bin u-boot.img u-boot.dtb FORCE
-	$(call if_changed,binman)
+OBJCOPYFLAGS_u-boot-sunxi-with-spl.bin = -I binary -O binary \
+				--pad-to=$(CONFIG_SPL_PAD_TO) --gap-fill=0xff
+u-boot-sunxi-with-spl.bin: spl/sunxi-spl.bin u-boot.img FORCE
+	$(call if_changed,pad_cat)
 else
 u-boot-sunxi-with-spl.bin: spl/sunxi-spl.bin u-boot.itb FORCE
 	$(call if_changed,cat)
--- a/arch/arm/Kconfig
+++ b/arch/arm/Kconfig
@@ -962,7 +962,6 @@ config ARCH_SOCFPGA
 
 config ARCH_SUNXI
 	bool "Support sunxi (Allwinner) SoCs"
-	select BINMAN
 	select CMD_GPIO
 	select CMD_MMC if MMC
 	select CMD_USB if DISTRO_DEFAULTS
