From 1da1aae0b207d6a5ac7c3070b8d7c6ef61a32d71 Mon Sep 17 00:00:00 2001
From: Claudiu Beznea <claudiu.beznea@microchip.com>
Date: Mon, 23 Aug 2021 16:19:14 +0300
Subject: [PATCH 225/247] ARM: dts: at91: sama7g5: add securam node

Add securam node.

Signed-off-by: Claudiu Beznea <claudiu.beznea@microchip.com>
Signed-off-by: Nicolas Ferre <nicolas.ferre@microchip.com>
Link: https://lore.kernel.org/r/20210823131915.23857-4-claudiu.beznea@microchip.com
---
 arch/arm/boot/dts/sama7g5.dtsi | 11 +++++++++++
 1 file changed, 11 insertions(+)

--- a/arch/arm/boot/dts/sama7g5.dtsi
+++ b/arch/arm/boot/dts/sama7g5.dtsi
@@ -75,6 +75,17 @@
 		#size-cells = <1>;
 		ranges;
 
+		securam: securam@e0000000 {
+			compatible = "microchip,sama7g5-securam", "atmel,sama5d2-securam", "mmio-sram";
+			reg = <0xe0000000 0x4000>;
+			clocks = <&pmc PMC_TYPE_PERIPHERAL 18>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0 0xe0000000 0x4000>;
+			no-memory-wc;
+			status = "okay";
+		};
+
 		secumod: secumod@e0004000 {
 			compatible = "microchip,sama7g5-secumod", "atmel,sama5d2-secumod", "syscon";
 			reg = <0xe0004000 0x4000>;
