// SPDX-License-Identifier: GPL-2.0-or-later

#include "rtl8380_netgear_gigabit_1xx.dtsi"

#include <dt-bindings/leds/common.h>

/ {
	compatible = "netgear,gs108t-v3", "realtek,rtl838x-soc";
	model = "Netgear GS108T v3";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_amber;
	};

	leds {
		compatible = "gpio-leds";

		led_power_amber: led-0 {
			label = "amber:power";
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_POWER;
			gpios = <&gpio1 32 GPIO_ACTIVE_LOW>;
		};

		led_power_green: led-1 {
			label = "green:power";
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			gpios = <&gpio1 31 GPIO_ACTIVE_LOW>;
		};
	};
};
