From 935d9aae15ee245a1bc6e322cbef02566a8996cc Mon Sep 17 00:00:00 2001
From: Claudiu Beznea <claudiu.beznea@microchip.com>
Date: Wed, 9 Dec 2020 15:03:34 +0200
Subject: [PATCH 117/247] net: macb: add function to disable all macb clocks

Add function to disable all macb clocks.

Signed-off-by: Claudiu Beznea <claudiu.beznea@microchip.com>
Suggested-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/cadence/macb_main.c | 38 +++++++++++++-----------
 1 file changed, 21 insertions(+), 17 deletions(-)

--- a/drivers/net/ethernet/cadence/macb_main.c
+++ b/drivers/net/ethernet/cadence/macb_main.c
@@ -3599,6 +3599,20 @@ static void macb_probe_queues(void __iom
 	*num_queues = hweight32(*queue_mask);
 }
 
+static void macb_clks_disable(struct clk *pclk, struct clk *hclk, struct clk *tx_clk,
+			      struct clk *rx_clk, struct clk *tsu_clk)
+{
+	struct clk_bulk_data clks[] = {
+		{ .clk = tsu_clk, },
+		{ .clk = rx_clk, },
+		{ .clk = pclk, },
+		{ .clk = hclk, },
+		{ .clk = tx_clk },
+	};
+
+	clk_bulk_disable_unprepare(ARRAY_SIZE(clks), clks);
+}
+
 static int macb_clk_init(struct platform_device *pdev, struct clk **pclk,
 			 struct clk **hclk, struct clk **tx_clk,
 			 struct clk **rx_clk, struct clk **tsu_clk)
@@ -4661,11 +4675,7 @@ err_out_free_netdev:
 	free_netdev(dev);
 
 err_disable_clocks:
-	clk_disable_unprepare(tx_clk);
-	clk_disable_unprepare(hclk);
-	clk_disable_unprepare(pclk);
-	clk_disable_unprepare(rx_clk);
-	clk_disable_unprepare(tsu_clk);
+	macb_clks_disable(pclk, hclk, tx_clk, rx_clk, tsu_clk);
 	pm_runtime_disable(&pdev->dev);
 	pm_runtime_set_suspended(&pdev->dev);
 	pm_runtime_dont_use_autosuspend(&pdev->dev);
@@ -4690,11 +4700,8 @@ static int macb_remove(struct platform_d
 		pm_runtime_disable(&pdev->dev);
 		pm_runtime_dont_use_autosuspend(&pdev->dev);
 		if (!pm_runtime_suspended(&pdev->dev)) {
-			clk_disable_unprepare(bp->tx_clk);
-			clk_disable_unprepare(bp->hclk);
-			clk_disable_unprepare(bp->pclk);
-			clk_disable_unprepare(bp->rx_clk);
-			clk_disable_unprepare(bp->tsu_clk);
+			macb_clks_disable(bp->pclk, bp->hclk, bp->tx_clk,
+					  bp->rx_clk, bp->tsu_clk);
 			pm_runtime_set_suspended(&pdev->dev);
 		}
 		phylink_destroy(bp->phylink);
@@ -4873,13 +4880,10 @@ static int __maybe_unused macb_runtime_s
 	struct net_device *netdev = dev_get_drvdata(dev);
 	struct macb *bp = netdev_priv(netdev);
 
-	if (!(device_may_wakeup(dev))) {
-		clk_disable_unprepare(bp->tx_clk);
-		clk_disable_unprepare(bp->hclk);
-		clk_disable_unprepare(bp->pclk);
-		clk_disable_unprepare(bp->rx_clk);
-	}
-	clk_disable_unprepare(bp->tsu_clk);
+	if (!(device_may_wakeup(dev)))
+		macb_clks_disable(bp->pclk, bp->hclk, bp->tx_clk, bp->rx_clk, bp->tsu_clk);
+	else
+		macb_clks_disable(NULL, NULL, NULL, NULL, bp->tsu_clk);
 
 	return 0;
 }
